ARES

EMERGENCY
 ALERTING PROCEDURE

MONITOR:

Primary  Repeater: 				146.7300
Primary   Simplex:				146.4750
Secondary Repeater				146.6400 or 145.1700/147.390

All ARES members may not be able to get into a certain repeater. So we will have to have stations that can operate on more than one repeater to put out the word of the alert status. The County EOC now has 2 repeater capability with the new two band VHF radio that has been installed. 

ALERT
CONDITIONS

LEVEL 0 - GREEN			NORMAL CONDITIONS

LEVEL 1 - YELLOW			POTENTIAL EXISTS FOR CALLOUT

LEVEL 2 - ORANGE			ON STAND-BY

LEVEL 3 - RED			ACTIVATED

LEVEL 4 - BLUE			DEACTIVATED